0 5 10 15 20 25 30 35 40 45 50 0

0.1

0.2

0.3

0.4

0.5 ME8192IV 0.8 dB code simulation

iteration number fraction of incorrect messages (check to variable)